# 3D Printing Summary

|  |  |
| --- | --- |
| **Metrics** |  |
| Total Print Time (min) | 38 |
| Total Number of Components | 1 |
| Typical Total Mass (g) | 5 |
| Typical Number of Print Setups | 1 |

# 3D Printing Settings

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Print File Name** | **Qty** | **Total Print Time (hr:min)** | **Mass (g)** | **Infill (%)** | **Support** | **Layer Height/ Nozzle Diameter(mm)** | **Notes (orientation, special settings, etc.)** |
| Beverage\_Can\_Opener.stl | 2 | 0:38 | 5 | 20 | No Support | 0.2/0.4 | * Must include at least 2 perimeters. * Ensure the print is oriented so that the flat side is laying on the print bed. |

# Post-Processing

* Check for sharp edges and burrs. Remove as needed.

# Customization Options

* Can be printed in any colour

# Example of a Quality Print

